GY50

Module gyroscope 3 axes

Chip: L3G4200D;

Power supply :3~5V;

Communication methods: IIC / SPI communication protocol;

Measuring range: 250 / 500 / 2000 dps

Application For gaming, virtual reality input device, motion control , HMI, GPS, electrical equipment and robotics

https://github.com/pololu/l3g-arduino